

**60% of all reported injuries in Chevron this year**

**are slips, trips and falls**

  

  

 

 **\* Vehicle cabs (in and out)**

 **Always 3 points of contact**

 **\* Flat bed of trucks**

 **Guard rails must be in place at all times, except when the vehicle is**

 **stationary, and then only when equipment is being loaded or off loaded**

  **\* Verge & centre reserve (long grass)**

 **Look out for kerbs; beware in long grass of discarded TM frames,**

 **pot holes, uncovered excavations, manholes or inspection chambers**

  **\* Safety boots**

 **Are laces tied properly; are boots fit for purpose?**

Watch your Step!



25 Nov 2011